Kenwood Remote control and Cross band repeating

Key (represented below as "xxx") is mother's birth month and day without leading zeros  
  
=== Repeat remotely  
Mobile:  
A to UHF  
B to VHF  
Select B  
Power off  
Hold REV and power on  
  
HT:  
Hold PTT  
Push Menu  
Rotate to Rpt On (Axxx#CA#)  
Push Menu  
Once dialing starts, release PTT  
  
---  
HT:  
Same as above, for Rpt Off (Axxx#DA#)  
  
Mobile:  
Same as above  
  
=== Repeat locally  
Mobile:  
Tune either frequency, one to UHF, other to VHF  
Either can be selected  
Power off  
Hold TONE and power on  
  
---  
Mobile:  
Same as above