Kenwood Remote control and Cross band repeating

Key (represented below as "xxx") is mother's birth month and day without leading zeros

=== Repeat remotely
Mobile:
A to UHF
B to VHF
Select B
Power off
Hold REV and power on

HT:
Hold PTT
Push Menu
Rotate to Rpt On (Axxx#CA#)
Push Menu
Once dialing starts, release PTT

---
HT:
Same as above, for Rpt Off (Axxx#DA#)

Mobile:
Same as above

=== Repeat locally
Mobile:
Tune either frequency, one to UHF, other to VHF
Either can be selected
Power off
Hold TONE and power on

---
Mobile:
Same as above